SimpleModbusSlave\_README

16/02/2014 - SMSv9

1. Cleaned up comments and changed the BUFFER size to 64 which matches the new buffer value in the hardwareSerial core library in version 1.05 onwards.

2. Added: void modbus\_update\_comms(long baud, unsigned char byteFormat, unsigned char \_slaveID);

This allows for easy update of the port variables and the slave id dynamically in your code.

10/11/2014 - SMSV10

Added function 6

The library for the DUE differs only in the removal of the byteFornat parameter in modbus\_configure().